**PURCHASE SPECIFICATIONS FOR A RUBBER PAD FOR SP-401 PORTABLE LIGHTING UNIT**

Rubber pad is designed to firmly place SP-401 portable lighting unit on different types of surfaces.

* Shall be made of high quality, thick rubber plate,
* Shall be applicable for any kind of surfaces (e.g. asphalt, concrete, grass or tarmac),
* Shall have lifespan of minimum 10 years,
* Shall be designed in such a way that SP-401 portable lighting unit mounted and fixed on the rubber pad could withstand jet blast of 240 kph. Compliance shall be confirmed by test report,
* Shall be equipped with latches allowing fast fixing and fast release of SP-401 portable lighting unit on the rubber pad.